aMTP32M supports 8bit mono wave format from 200 sec(best quality) ~ 660 sec. We offer 2 software for choose.

.imEDIT_VXXX:
 It supports any wav format files. Quickly to guide user to finish programming.

.aSPI28W_VXXX:
 It allows user to load 8 bit mono wave with different sample rate from 6k~20Khz. Usually it is for experienced user
 who can do editing himself.

How to use imEDIT_VXXX or aSPI28W_VXXX ?
Step 1 : Copy directory "Software" files to HDISK.
Step 2 : aSPI28W Writer install 
         .see the document for imEDIT_VXXX: X:\aMTP32M CD\Software\imEdit_V201\GettingStarted.html
         .see the document for aSPI28W_VXXX: X:\aMTP32M CD\Software\aSPI28W_V100\Doc\aSPI28W-UserGuide_V1.2_20120106.pdf
Step 3 : Double click X:\aMTP32M CD\Software\imEdit_V100\imEdit.exe to run or
         Double click X:\aMTP32M CD\Software\aSPI28W_V100\aSPI28W.exe to run

Contact me for any help : 
     
Home page : http://www.aplusinc.com.tw
E-mail : edit@aplusinc.com.tw
skype : xyz_steven
Written by Steven Lin of Aplus Integrated circuit INC.