imEdit Getting Started

[ Windows XP ]
[ Windows 7 ]

Windows XP

1. Connect aSPI28W to your computer by USB cable.

2. When first time connect aSPI28W to the computer, windows will show ˇ§Found New Hardware Wizardˇ¨ windows, select [ No, not this time ] , then click [ Next ] .

3. Select [ Install from a list or specific location (Advanced) ] , then click [ Next ] .

4. Select [ Include this location in the search ] and click [ Browse... ] .

5. Select the "Driver" folder which under your install directory, then click [ OK ] .

6. Click [ Next ] .

7. Windows will copy the driver to your PC and start to install.

8. Click [ Finish ] to end of install driver.

9. Now, double click imEdit icon to start the software.

[ TOP ]

Windows 7

1. Connect aSPI28W to your computer by USB cable.

2. Click and follow below graph to open [ Control Panel ]

3. Click and follow below graph to open [ Hardware and Sound ] .

4. Click and follow below graph to open [ Device Manager ] .

5. You can find aMTP32M in the list.

6. Right-click aMTP32M icon, and click [ Update Device Software... ].

7. Click and follow below graph to install driver manually.

8. Select [ Include subfolders ] and click [ Browse... ] .

9. Select the "Driver" folder which under your install directory, then click [ OK ] .

10. Click [ Next ] .

11. Windows will start to install driver to your PC.

12. When the driver install, if windows show the below message, please click [ Install this driver software anyway ] .

13. Click [ Close ] to end of install driver.

14. Now, double click imEdit icon to start the software.

[ TOP ]